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Visual Display Units
PART 1 GENERAL
1.01 SECTION INCLUDES
A. Glass Marker Wall.
1.02 REFERENCE STANDARDS
A. 16 CFR 1201 - Safety Standard for Architectural Glazing Materials; Current Edition.
B. ANSI Z97.1 - American National Standard for Safety Glazing Materials Used in Buildings - Safety Performance Specifications and Methods of Test; 2015 (Reaffirmed 2020).
1.03 SUBMITTALS
A. Product Data: Provide manufacturer's data on Glass Marker Wall Covering. Include Material Safety Data Sheets when applicable
B. Shop Drawings: Submit shop drawings for each type of visual display board as specified, including sectional details, trim, face and core materials, dimensions, joint locations, and any special anchor details. , special anchor details
C. Color Samples: Provide a complete set of color swatches showcasing the manufacturer's full selection of colors and finishes for Tackable Wall Covering
D. Products Samples: Two​, 10" by 10" inches [254 by 254] mm in size illustrating materials and finish, color and texture of tackable surfaces.
E. Manufacturer's printed installation instructions.
1.04 QUALITY ASSURANCE
A. Manufacturer Qualifications: Company specializing in manufacturing the products specified in this section with minimum 20 years documented experience
1.05 WARRANTY
A. Provide the manufacturer's standard three-year warranty for workmanship, confirming that, with proper usage, maintenance, and installation according to the manufacturer's guidelines, the Glass Marker Wall are guaranteed for three-year from the date of substantial completion.
PART 2 PRODUCTS
2.01 MANUFACTURERS
A. ​Visual Display Units
1. Nelson Adams NACO
2. Address: 420 S. E St. San Bernardino CA 92401
3. P: (877) 810-4080
4. Web Page: https://nelsonadamsnaco.com
2.02 GLASS MARKER WALL
A. ​Magnetic ​Glass Markerboard Wall: Room-size presentation surface made of multiple ​floor-to-celing​ glass panels.
1. Glass: ​​​Back-coated glass​​​, ​​​tempered, low iron​​​, ​​​1/4 inch thick (6 mm)​​​, ​​​with flat polish and square corners​​​​​​, laminated to steel backing sheet for use with magnets​​​. Coated or treated for use as ​​​dry-erase board​​​.
2. Glass Finish: ​​​As selected from manufacturer's full range​​​.
3. Steel Backing Sheet Thickness: 24 gauge, 0.0239 inch  (0.61 mm).
4. Panel Width: ​​48 inches (1220 mm)​​.
5. Height: ​​​As indicated on drawings​​​.
6. Length: ​​​As indicated on drawings​​​.
7. Accessories: Provide ​​​magnetic marker tray, magnetic marker holder, and [magnetic eraser]​​​.
2.03 MATERIALS
A. Glass: Provide glass-based glazing unless otherwise indicated.
1. Fully Tempered Safety Glass:  Comply with ANSI Z97.1 or 16 CFR 1201 criteria for safety glazing used in hazardous locations.
2.04 ACCESSORIES
A. Temporary Protective Cover: Sheet polyethylene, ​​8 mil (0.2 mm)​​ thick.
B. Magnetic Tray: Aluminum, manufacturer's standard profile, one piece full length of markerboard, molded ends, concealed fasteners, same finish as frame.
C. Magentic eraser: dry-erase board cleaning accessory with an integrated magnet that allows it to attach directly to magnetic glass board surfaces.
PART 3 EXECUTION
3.01 EXAMINATION
A. Verify that field measurements are as indicated.
B. Verify that internal wall blocking is ready to receive work and positioning dimensions are as indicated on shop drawings.
3.02 PREPARATION
A. Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
3.03 INSTALLATION
A. Install boards in accordance with manufacturer's instructions.
B. Secure units level and plumb.
C. Mounting: [ Concealed Z clips ][ Stainless Steel Standoffs ]
3.04 CLEANING
A. Clean board surfaces in accordance with manufacturer's instructions.
B. Cover with protective cover, taped to frame.
C. Remove temporary protective cover at Date of Substantial Completion.
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